**TECHNICAL SPECIFICATIONS**

|  |  |  |  |
| --- | --- | --- | --- |
| **Item #** | **IOM’S SPECIFICATIONS – MINIMUM REQUIREMENTS** | **BIDDER'S SPECIFICATIONS include photo reference** | **Indicate**  **COMPLY or NOT Comply** |
| 1 | Technical BCD donut wing 1680 Denier Ballistics, Back Plate S.S. 3mm, Back Pad with Pocket, two side pocket for inner Bladder 420 Denier, Solo Harness with s.s. D-ring, two cam band weight, single tank adapter, inner Bladder 420 Denier, Solo Harness with s.s. D-ring, two can bank. |  |  |
| 2 | Dive computer, three mixes O2, three Dive modes (scuba, free, gauge).  Two algorithms (Buhlman and DSAT) easy to change battery CR 2450 with screen guard – Bluetooth. |  |  |
| 3 | Aluminum alloy scuba-diving tank S080 with Thermo Nitrox Valve 11.1 liters 230 BAR working pressure. |  |  |
| 4 | Regulator Nitrox 300 Bar Din, piston regulated, un-balanced, 1st and 2nd stage with hose, 5 ports, 2 HP and 3 LP. |  |  |
| 5 | Silk rope 14mm 100m |  |  |
| 6 | Octopus 2nd stage with 90cm hose and snap bolt, color: yellow. |  |  |
| 7 | Gauge 3 element SPG, Depth gauge and Compass with HP hose tested 1650 BAR. |  |  |
| 8 | Wetsuit 3mm, neoprene, one piece, stretch, comfortable & durable with ankle zip. |  |  |
| 9 | Wet suit 5mm stretch with ankle zip. |  |  |
| 10 | Vest 3mm, with Hood 5mm Stretch and Merino wool inside for cold water. |  |  |
| 11 | Diving knife S.S. Blade 11cm black with two straps. |  |  |
| 12 | Frameless mask with silicone black big eye low volume tempered glass, single lenses, frameless, low volume. |  |  |
| 13 | Snorkel full silicone foldable. |  |  |
| 14 | Fins adjustable, open heel, 70cm, heavy-duty, adjustable with quick release, buckle color black. |  |  |
| 15 | Diving boots, heavy duty, neoprene with zip 5mm rubber sole with additional heel cap for protection. |  |  |
| 16 | Diving torch aluminum Led 1900 lumen lithium battery with USB charge, three modes, 150mt. Depth with extra button till 3000 lumens. |  |  |
| 17 | Diving gloves 2.5mm super-stretch Neoprene with finger and palm reinforcement color black. |  |  |
| 18 | Mech bag for diving equipment, with shoulder Pad handles, Rugged construction, 100 liters. |  |  |
| 19 | BCD hanger multipurpose. |  |  |
| 20 | Spool with double ended s.s. 30mt with strong cord of 80 kg. |  |  |
| 21 | Marker Buoy 130cm with dump valve inflate by regulator and by mouth. |  |  |
| 22 | Lift bag 1000kg polyurethane with s.s. Dring, Rugged Construction. |  |  |
| 23 | Dry suit telescopy excellent durability and abrasion-resistance with CORDURA Nylon Oxford 4-layer fabric and a lightweight, breathable with side pocket and including Rock Boot. |  |  |

## \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

## Supplier’s authorized signature over printed name