**TECHNICAL SPECIFICATIONS**

|  |  |  |
| --- | --- | --- |
| **IOM’S SPECIFICATIONS** | **BIDDER'S SPECIFICATIONS** | **Indicate** **COMPLY or NOT Comply** |
| **Passenger Minibus*** Wheelbase 3275 ± 300 mm, RWD or FWD is acceptable
* Manual Transmission
* Engine Type: Diesel
* ≤9 seats (Ukrainian category B driving license)
* Road clearance ≥150 mm
* Left-side steering wheel with power steering
* Engine ≥90 kW, diesel or petrol, EURO4 or better, ≥70 l fuel tank with a cap lock
* Set of winter M+S tires, incl. spare
* Set of summer tires, incl. spare
* White color

ABS, ESC, A/C, seatbelts for all seats, 12V plug, 2 front airbags, fire extinguisher (2 l or more), first aid kit (as required by Ukrainian legislation), rear tow-hook, driver`s tool kit (incl. two emergency stop signs), set of spare plugs (in case of petrol engine), 4 retaining nuts for wheels, set of spare lamps (headlights and fender lamps), fog light, radio, rear window heating, lower back panels, remote central locking, maintenance manual in Ukrainian or Russian (one hard copy per vehicle and a soft copy of all documents).**Warranty, After-sales services, and Technical Training**Warranty: Should be able to provide two options for the minibuses within Ukraine or the regionOption1: 1-year standard manufacturing warranty Option2: 3 years standard manufacturing warrantyAfter-sales services: Should be able to offer local or regional after-sales support if local support is not available. |  |  |
|  |  |  |

## \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

## Supplier’s authorized signature over printed name