**TECHNICAL SPECIFICATIONS**

|  |  |  |
| --- | --- | --- |
| **IOM’S SPECIFICATIONS** | **BIDDER'S SPECIFICATIONS** | **Indicate**  **COMPLY or NOT Comply** |
| **Folding Ladders Wooden ladder** / Swedish Wooden raw material, quality raw material with coating, loading capacity 150Kg.  Size: 6 feet  سلم خشب سويدي |  |  |
| **Long scissors for trees / مقص ليمون يد طويلة**  Durable Tree Cutting Scissors Long Handle Pruning Garden Shear With High Quality.  Anti-Slip Grip, Folding.  Cutting Capacity: 1 inch  Blade Length: 3 inches  Cutting diameter: 0-40mm  Material: SK5 (Carbon Steel)  Handle: PVC  Size: 680-1005mm  Application: Trees  Finishing: chrome plated |  |  |
|  |  |  |
| **Electric Hedge trimmer / موتير قص ورق**  Electric Hedge Trimmer 20v With High-efficiency DC Motor  Power: 450W  Blade: Punch blade,65Mn double-sided  SPM:3200  Weight: approx. 5kg  Scissor Type: DUAL  Length Of Blade and Cutting length: 510MM  Power Source: Battery  No loading speed: 1400rpm  Max cutting capacity: 16mm |  |  |
| **Gasoline lawn mower threads / خيطان مكنة قص**  **عشب**  4-Stroke, Anti-slip, Folding Handle, Grass Box, Height Adjustable Hand  Cutting heights: 1.25in. to 3.75  Cutting Width 20 inches  Power Source: Gas Cutting  Number of cutting heights settings: 6  Drive Type: Self propelled  Oil Volume:0.4L  Catcher Capacity: 65L  Device material: Plastic & Metal  power Source: Petrol/Gasoline  Engine speed: 2800rpm  Gasoline tank volume: 1L  Deck Material: Steel  Height Adjustment: 25-70mm with 8 settings, central  Wheel: Front 178mm & rear 250mm |  |  |
| Water hose / نربيش سقاية  Diameter:  1/2",5/8'',3/4"  Hose material: PVC  Color: yellow, red or green  Adavantage: Anti-UV, Anti-Abrasion, Anti-Corrosion, Anti-UV, Flexible, Soft  Working Temperature: -10°C~+40°C  Size/diameter: 4 inches  Length: 30 feet |  |  |
| **Hand saw / منشار يد**  professional level Hand Saw 20inch/500mm High Quality Hand Saw Hand Saws For Cutting Trees  Application: Metal, wood, plastic  Teeth per Inch: 18  Blade Type: FIXED BLADE  Material: Steel and wooden wrist  Blade Length: 20inch  Dimensions: 500mm  Weight: approx. 0.60kg  Color: any  Length of saw blade: 300 |  |  |
| **Saw Blades / نسلات منشار**  Blade Width: 1.8mm  Teeths: 30  Blade Length: 6 1/2in  Blade Diameter: 4in  Edge Height: 0.315in(8mm)  Size: 110x1.8x20mm  Application: Wood  Material: Diamond Powder+Alloy Steel  Teeth type: BC Teeth  Color: Silver  Thickness: +/-.001” |  |  |
| **Engine Chain For Cutting Woods / جنزير موتير قص الحطب**  Engine Displacement: 25.4cc  Power: 1.0kw  2-Stroke, Forced Air Cooling, Single Cylinder  Power Source: Petrol/Gasoline  Engine type: Air Cooled, 2 Stroke Single Cylinder Gasoline  Rated Output Power&Relevant Speed: 1. 0kw  Fuel Mixture Ratio: 25/1(Gasoline 25: Two-cycle Oil 1)  Fuel Tank Capacity: 230ml  Engine Oil Tank Capacity: 160ml  Guide Bar: 10''  Net Weight: approx. 3.2kg  Type: Handheld  Power: gasoline?  Blade type: Dual  Brake: mechanic  Operation Mode: Double Action |  |  |
| Paper Clips / ملقط اوراق  Small around 22mm  Material: Metal |  |  |
| **rough comb / مشط خشن**  Size: 203mm  Handle Material: 66 nylon, carbon 30% |  |  |
| **Soft Comb / مشط ناعم** |  |  |
| **Large lawn mower head / رأس ماكينة الخيط لقص العشب الكبيرة**  Volt Brushless Self-Propelled Mower. It holds its own against gas-powered models, has a 20-inch deck that mulches and bags, and an optional side-discharge chute (sold separately). It can run for up to 40 minutes per charge. |  |  |
| **Small Rake / منكوش صغير**  Handle length: 150cm  Working width: 36cm  Wooden handle  Head Material: Steel  Handle Material: Wood |  |  |
| **Plastic roller Bin / عرباية نفايات بلاستيك**  Corrosion resistant, No absorption, Stackable.  Material: Plastic  Size: 360L  *A green garbage can  Description automatically generated with medium confidence* |  |  |
| **Large scissors / مقص كبير**  Material: stainless steel  Blade Length: 4 inch |  |  |
| **Felco or equivalent**  **small scissors blade / شفرة مقص صغير**  Size: 215mm  Material: steel  Finishing: Not Coated  Max Cutting Capacity: 22mm |  |  |
| **Backpack sprayer for pesticides / مرشه ظهر للمبيدات**  Capacity: 16L  Gross weight: 5.5KG  Nozzle: flat  Type: electric |  |  |
| **Shovel / مجرفه**  Blade Length:  8in  Blade material: Drop forged Carbon Steel  Total length: 39"/1m  Handle Type: D-Grip  Style: Round shovel  Handle material: 1st grade wood handle |  |  |
| Paint / Black (tinol or similar) for sidewalks (4 KG) |  |  |
| Paint / Phosphore (tenol or similar) for sidewalks (4 KG) |  |  |
| Paint / white(tenol or similar) for sidewalks (4 KG) |  |  |
| turpentine (bottle)  volume: 1L |  |  |
| Paint Roller /Large |  |  |
| Paint Roller/Small |  |  |
| Paint brush, Size 4  *A picture containing tool, broom  Description automatically generated* |  |  |
| Broom /Large for road sides (Heavy Duty)  Handle: wooden  Brush handle 120\*2cm, brus 40\*6\*2cm, 7.5cm bristle |  |  |
| Broom / thin (Heavy duty)  Handle: cabon  Single package size:  150X6X7.5 cm  Single gross weight:  3.000 kg |  |  |
| Paint Paste (Galons) |  |  |
| Wall Scraper, Size 4  *A picture containing tool  Description automatically generated* |  |  |
| Water tap (neck type)  Turkish brand or similar/equivalent |  |  |
| Water mixer  Turkish brand or similar/equivalent  Function: Hot Cold Water  Surface Treatment: Polished  Cartridge: 35mm Ceramic Cartridge  *A close-up of a stethoscope  Description automatically generated with medium confidence* |  |  |
| Water riser for toilet  Turkish brand or similar /equivalent |  |  |

## \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

## Supplier’s authorized signature over printed name